# SES 1 @ 101.0W C-BAND
# freq pol sr fec

[CHANNEL]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 4020000
	POLARIZATION = HORIZONTAL
	SYMBOL_RATE = 28000000
	INNER_FEC = 3/4
	MODULATION = PSK/8
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 3715000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 4775000
	INNER_FEC = 3/5
	MODULATION = PSK/8
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3720000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 10000000
	INNER_FEC = 5/6
	MODULATION = QPSK
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3773000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 4441000
	INNER_FEC = 3/4
	MODULATION = QPSK
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3952000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 2734000
	INNER_FEC = 5/6
	MODULATION = QPSK
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3956000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 2734000
	INNER_FEC = 5/6
	MODULATION = QPSK
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3960000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 2734000
	INNER_FEC = 5/6
	MODULATION = QPSK
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3973000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 5924000
	INNER_FEC = 5/6
	MODULATION = QPSK
	INVERSION = AUTO

