# AMC 10 @ 135W C-BAND
# freq pol sr fec

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3820000
	POLARIZATION = HORIZONTAL
	SYMBOL_RATE = 29268000
	INNER_FEC = 3/4
	MODULATION = QPSK
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3900000
	POLARIZATION = HORIZONTAL
	SYMBOL_RATE = 29268000
	INNER_FEC = 3/4
	MODULATION = QPSK
	INVERSION = AUTO

