# Australia / Wollongong
#
# Australia modulation params:
# - http://www.dba.org.au/index.asp?sectionID=120
#
#
# North (Broadcast Site Escarpment Road BROKERS NOSE)
# - http://www.dba.org.au/index.asp?query=true&sectionID=22&recLocation=Wollongong+%2D+North
#
# ABC UHF52
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 697500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Prime UHF46
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 655500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# WIN UHF40
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 613500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Ten UHF43
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 634500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS UHF54
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 711625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

#
# Illawarra (Broadcast Australia Digital Television Tower KNIGHTS HILL)
# - http://www.dba.org.au/index.asp?query=true&sectionID=22&recLocation=Wollongong+%2D+Illawarra
#
# ABC UHF51
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Prime UHF38
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 599500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# WIN UHF36
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 585500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Ten UHF37
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 592500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS - same as North
#
# Stanwell Park (Bald Hill STANWELL TOPS)
# - http://www.dba.org.au/index.asp?query=true&sectionID=22&recLocation=Wollongong+%2D+Stanwell%20Park
#
# ABC, Prime, WIN, Ten are identical to Wollongong / North
# SBS UHF49
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 676500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

